* 1. **New Model**
     1. Approval

1. Prior to mass production start and delivery, new model product must be approved by WCP.
2. Approval requirements include but are not limited to…
3. Level 3 PPAP including but not limited to…
4. Supporting data including “A-B” (previous vs proposed) capability study data.
5. Updated control plans and FMEA reflecting the controls for the proposed changes.
6. Functional and/or safety confirmation data...

*NOTE: Any new model product, which (as determined by WCP) requires verification by WCP and/or design/testing*

*resources available to WCP), is subject to testing fees, which will be the responsibility of the product supplier.*

1. Additional approval requirements may include, but are not limited to.
2. A QAV (Quality Assurance Visit) by WCP to the supplier’s location to verify the controls relative to the proposed change.
   * 1. Formal approval of the new model product is identified by the supplier’s receipt of the previously submitted Warrant as level 3 PPAP “Warrant”, which contains a WCP judgment of “APPROVED” and corresponding WCP approval signature.
   1. **Labeling**

6.2.1 Format

1. All received shipments shall be labeled with labeling conformant to AIAG B-10 requirements.
2. All labels must include at minimum the following information….
3. WCP part number as indicated on the P.O.
4. Ship from (supplier) information
5. Quantity
6. Product serial number (when applicable)
7. Manufacturer’s lot number
8. Color (when applicable)
9. Customer part number (when directed by WCP).
10. Product Description.
    * 1. Placement
11. All product shall have label(s) applied to each container and/or skid/rack of product as per arranged packaging agreement.